Jong, T. (2006). Microbial sulfate reduction under sequentially acidic conditions in an upflow anaerobic packed bed bioreactor. Water Research, 40(13), 2561–2571.