Wiessner, A. (1998). The treatment of a deposited lignite pyrolysis wastewater by adsorption using activated carbon and activated coke. Colloids and Surfaces a-Physicochemical and Engineering Aspects, 139(1), 91–97.