Bureau of Mines, U. S. D. of the I. (1991). Accelerated pyrite oxidation/enhanced alkalinity couple to reduce acid mine drainage.